2) Base-emitter current: 3.82mA

Collector-emitter current: 84.3mA